--lpm_abs CARRY_CHAIN="MANUAL" DEVICE_FAMILY="Cyclone V" IGNORE_CARRY_BUFFERS="OFF" LPM_WIDTH=4 data result
--VERSION_BEGIN 23.1 cbx_cycloneii 2023:11:29:19:33:06:SC cbx_lpm_abs 2023:11:29:19:33:06:SC cbx_lpm_add_sub 2023:11:29:19:33:06:SC cbx_mgl 2023:11:29:19:43:53:SC cbx_nadder 2023:11:29:19:33:06:SC cbx_stratix 2023:11:29:19:33:06:SC cbx_stratixii 2023:11:29:19:33:05:SC cbx_util_mgl 2023:11:29:19:33:06:SC  VERSION_END


-- Copyright (C) 2023  Intel Corporation. All rights reserved.
--  Your use of Intel Corporation's design tools, logic functions 
--  and other software and tools, and any partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Intel Program License 
--  Subscription Agreement, the Intel Quartus Prime License Agreement,
--  the Intel FPGA IP License Agreement, or other applicable license
--  agreement, including, without limitation, that your use is for
--  the sole purpose of programming logic devices manufactured by
--  Intel and sold by Intel or its authorized distributors.  Please
--  refer to the applicable agreement for further details, at
--  https://fpgasoftware.intel.com/eula.



--synthesis_resources = lut 3 
SUBDESIGN lpm_abs_jn9
( 
	data[3..0]	:	input;
	overflow	:	output;
	result[3..0]	:	output;
) 
VARIABLE 
	result_tmp[3..0]	: WIRE;

BEGIN 
	overflow = (result_tmp[3..3] & data[3..3]);
	result[] = result_tmp[];
	result_tmp[] = ( (data[3..3] & (! ((data[2..2] # data[1..1]) # data[0..0]))), (((data[2..2] $ (data[1..1] # data[0..0])) & data[3..3]) # (data[2..2] & (! data[3..3]))), (((data[1..1] $ data[0..0]) & data[3..3]) # (data[1..1] & (! data[3..3]))), data[0..0]);
END;
--VALID FILE
